**Z-800F Infusion Pump Patient Guide**

* Power on Pump by pressing ON/OFF key for 2 seconds.

**Prepare Tubing**: Do not use prime button to prime tubing.

* Spike bag and PRIME tubing by gravity **before loading into pump**. Squeeze drip chamber 2/3 full, then slowly open roller clamp to prime. After tubing is primed engage both the roller clamp and white clamp.

**Load Set**

* Open door of pump.
* With thumb, press green button and slide white clamp, with wings facing up, into loading module.

****

* With fingertip, push tubing into guides, and into black air sensor, aligning tubing on top of Pump based free flow clamp at the bottom. **Do not force tubing into clamp.**
* Secure door by pushing down on door handle.

**Choose New Infusion** by highlighting using arrow, press OK. Then input infusion program.

* Choose either: (by highlighting)
	+ Cont Mode R/V
	+ Cont Mode T/V
	+ TPN mode
* Press SELECT

**Pri Rate 0000**  means primary rate of infusion. Use the number keys 100-10-1 to input rate.

(Example: Rate of infusion 166 = Press 100 once + 10 six times + 1 six times)

**Pri VTBI 0000** means Primary volume to be infused. Highlight by pressing the **.**

Use number keys 100-10-1 to input volume. (Example: Volume to be infused 250 = 100 twice + 10 five times)

**Press Run/Stop to start infusion.**

**To power OFF press ON/OFF key for 2 seconds.**